Paper Handling

# Loading Passbooks

You can load vertical-fold and horizontal-fold passbooks. Follow the steps shown below to load passbooks.

| Note:

The illustrations in this manual are slightly different than LQ-690K. However, the explanations are the same.

| Turn on the printer.

| Open your passbook to the page to be printed.

|  | Note:

Make sure that you press any bulging parts of the folded passbook down to 0.5 mm or less before inserting it into the front slot.

| Insert the passbook printable side up into the front slot until the top part of it reaches the roller inside. The left edge of the passbook is adjusted to where it is marked on left side of the edge guide. The printer loads it automatically to the correct position and the passbook is ready to be printed.

|  | Note:

Fully open the passbook before inserting it.

Remove the tractor unit on the backside of the printer so that the passbook can be printed.

| Caution:

To print a passbook, click the Tear off/Passbook button to turn on the passbook mode.

Set the paper-thickness lever to or .

To select Passbook, the platen gap switch must be at the second position or wider.

Use a passbook that has more than 60% reflectance.

Do not load passbooks that are creased or have ripped seam.

Do not use a passbook that has any metallic parts such as staplers or metal clips.

Do not use a passbook with sticky parts such as stamps or seals.

Do not use a passbook that has any pages smaller than the cover page.

Do not use a passbook that the reliability will be impaired, tear, crease, fold, or loose ofstitch.

Do not print on the front or back cover of a passbook. Printing can be done only when the passbook is opened.

Always close the printer cover before printing. The printer does not print when the printer cover is open.

The sprocket unit and paper support should be slided to the right side of the printer and be locked.

[Top]

Previous