Product Information

# Command Lists

> EPSON ESC/P-K control codes
> IBM PPDS emulation control codes
> OKI5530SC emulation control codes

Your printer supports the EPSON ESC/P-K control codes, IBM PPDS emulation and OKI5530SC emulation control codes listed below.

## EPSON ESC/P-K control codes

Selecting an EPSON ESC/P-K printer in your software allows you to use advanced fonts and graphics.

Operation control:
| CR
Format control:
| ESC 0, ESC 2, ESC 3, ESC A, ESC +, LF, ESC J, ESC C, ESC C NUL, FF, ESC N, ESC O, ESC B, VT, ESC Q, ESC l, ESC D, HT, ESC SP, ESC $, ESC \, ESC ( C, ESC ( c, ESC ( U, ESC ( V, ESC ( v, ESC ( P
Print variation control:
| SO, DC4, ESC W, SI, DC2, ESC E, ESC F, ESC G, ESC H, ESC w, ESC P, ESC M, ESC g, ESC p, ESC S, ESC T, ESC 4, ESC 5, ESC t, ESC 6, ESC 7, ESC !, ESC -, ESC ( -, ESC R, ESC x, ESC y, ESC q, ESC k, ESC %, ESC:, ESC &, ESC ( X, ESC X, ESC c, ESC ( ^, ESC ( t
Bit image:
| ESC K, ESC L, ESC Y, ESC Z, ESC *, ESC ?
Raster graphics mode control codes:
| ESC ( G, ESC .
Hanzi mode:
| FS &, FS ., FS SO, FS DC4, FS W, FS J, FS K, FS D (vertical printing), FS -, FS S, FS T, FS U, FS V (adjustment), FS x, FS 2, FS SI, FS DC2, FS r, FS v, FS k, FS !, FS y, FS ( I
CC-DOS control codes:
| ESC I A, ESC I B, ESC I C, ESC I D
Barcode:
| ESC ( B
Production command:
| ESC |
Other control:
| ESC @, BEL, BS, DEL, CAN, ESC U, DC1, DC3, ESC =, ESC >, ESC #

[Top]

## IBM PPDS emulation control codes

This printer emulates the IBM Proprinter using the commands below.

General operation: NUL, DC3, ESC j, BEL, CAN, DC1, ESC Q, ESC [ K, ESC U, ESC [ F
Paper feeding: FF, LF, ESC 5, ESC A, ESC A (AGM*), ESC 0, ESC 1, ESC 2, ESC 3, ESC 3 (AGM*), CR, ESC ]
Page format: ESC C, ESC C NUL, ESC X, ESC N, ESC O, ESC 4
Print position motion: ESC d, ESC R, ESC D, HT, ESC B, VT, ESC J, ESC J (AGM*)
Font selection: DC2, ESC P, ESC :, ESC E, ESC F, ESC I, ESC [d, ESC [I
Font enhancement: DC4, SO, ESC SO, ESC W, ESC [ @, SI, ESC SI, ESC G, ESC H, ESC T, ESC S, ESC -, ESC _, ESC [-
Spacing: BS, SP, ESC [\
Character handling: ESC 6, ESC 7, ESC [ T, ESC ^, ESC \
Bit image: ESC K, ESC L, ESC Y, ESC Z, ESC [g, ESC * (AGM*)
Bar code: ESC [f, ESC [p
Download: ESC = (command is not provided)

| * Alternate Graphic Mode

[Top]

## OKI5530SC emulation control codes

This printer emulates the OKI5530SC Proprinter using the commands below.

Printer control:
| DC1, DC3, ESC b, ESC k, ESC l, CAN, DLE B
Forms control:
| FF, LF, ESC 6, ESC 8, ESC % 9, ESC % 5, ESC VT
Page format:
| ESC F, ESC G, ESC 5, VT, DC 4
Carriage control:
| ESC % 3, ESC % 4, ESC % 6, HT, ESC L, ESC (, ESC ), BS, CR
Character control:
| CEX $, CEX N, CEX O, CEX P, CEX Q, CEX R, CEX S, ESC N, ESC H, ESC B, ESC E, ESC &, ESC \xd4 , ESC $ @, ESC (H, CEX r, CEX s, CEX 0, CEX 2, CEX J, CEX K, CEX _, CEX t, CEX u,
Bit image:
| ESC %1, ESC %2
Printing mode control:
| ESC D, ESC I, ESC O, ESC X, ESC Y, ESC U, ESC R, ESC g, ESC h, ESC <, ESC >, ESC ], ESC [, ESC e, ESC f, CEX p, CEX q, ESC i, ESC j,ESC m, ESC n, ESC % U, ESC % B

[Top]

Previous | Next